|  |  |  |
| --- | --- | --- |
| **Sl No.**  | **Particulars Description** **Scheme Code: CCCT/ACAF/RENO/01** | **Qty** |
| 1. | **Renovation and installation of badminton Mat of** **Badminton Hall.** |  |
| a) | Work: renovation of floor: Chipping of all floorsurface and reconstruction of floor with cementpolishing | 2500 |
| b) | Installation of Badminton Mat (Li-Lining) BWFCertified with Installation | 1 |
| c) | 2.5 mm cushion 8X4, good quality. Withinstallation of dendrite etc | 1 |
| 2. | **Renovation of Basketball area** |  |
| a) | Work: Renovation of Floor area and installation ofpaver block, as suggested (24 X 28) | 672 |
| 3. | **Renovation of Volleyball Court** |  |
| a) | Work: Volley Ball Court Renovation, Laying ofriver Sand and marking of lines with PVC Plank/Concrete Slab (Roller fare not included) | 1 |
| b) | **Repairing of Volleyball Pole** | 2 |
| c) | Boundry Fenching: (H 10 Ft X L 80 Ft X 2mm Día) with chain link fenching, with Iron angle pole:erection of pole etc. | 800 |
| d) | Pavellion Railing with 2.5 mm Mild Steel Sq Pipe(50 Ft X 3 Ft) | 150 |
| 4. | **Throw Ball Area** |  |
| a) | Fenching College Building area with 2mm ChainLink Fenching. (30 X 10) | 300 |
| b) | Boundry Fenching (H 10 Ft X L 25 Ft X 2mm Dia)with chain link fenching, with Iron angle pole: erection of pole etc. | 250 |
| 5. | **Football Ground** |  |
| a) | Sifting of Gole Post (Labour) | 2 |
| b) | Boundry Fenching: (H 10 Ft X L 50 Ft X 2mm Dia)with chain link fenching, with Iron angle pole:erection of pole etc. | 500 |
| 6. | **Office Installation and furnishing** |  |
| a) | Office Table with three drawer on RHS with squaretubular leg, foot rest and rubber shoe with soild prelaminated practical board top. | 1 |
| b) | Office Chair Visitor blue fabric upholstery with arm rest Model No RC6410 Rajkamal. (S Chair) | 3 |
| c) | Executive Chair, Mid Black Managerial ChairModel No RC 8711 Rajkamal | 1 |
| d) | Inveter, 1.5 Kva Microtech. 180 Ah Battery 2 Nos.with Installation and cabelling upto Badmintond) Hall As per survey done by engineer | 1 |
| **7.** | **Renovation and construction of Library** | 1 |
| **a)** | **Renovation of wall 46’ x 11’** |  |

**Note: Interested parties are requested to visit the site at CCCT, Chisopani, Namchi district, see the nature and quantity of work and place quotation within the given budget accordingly.**